SECTION A

INDEX TO MANUAL SECTIONS

CONTENTS

Page

Contents .. .. .. .. .. .. .. .. .. 3

Illustrations .. .. .. .. .. .. •• •• •• 6

Tables .\* »\* •• »» •• •• •• •• •• •• 17

CONTENTS

Foreword

Paxman Information Bulletin Service  
Distribution  
Safety Warnings

SECTION

1. **Index to Manual Sections**
2. **General Description**
3. **Technical Data**
4. Engine Data
5. Operating Data
6. Timing Operations
7. Schedule of Clearances and Wear Limits
8. Torque Loadings
9. **Operation**
10. Priming, Venting, Initial Starting Preparations, Starting and Stopping
11. Fault Finding
12. **Engine Maintenance Notes**
13. Maintenance Schedule
14. General Overhaul Notes
15. **Basic Engine Components**
16. Cylinder Heads and Valve Gear
17. Pistons, Connecting Rods Large and Small-end Bearings.

Including:

Addendum 200FB009 - Pistons and rings

1. Camshaft, Cam Followers and Bearings
2. Auxiliary Drives Gear Train
3. Crankshaft and Main Bearings
4. Torsional Vibration Dampers
5. Crankcase, Cylinder Liners, Free-end cover and Sump

LIMITED RIGHTS LEGEND

USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15.

SECTION

1. Fuel System
2. Fuel Oil Specification
3. Fuel Oil System
4. Fuel Feed Pump and Drive
5. Hand Operated Priming Pump
6. Fuel Reservoir
7. Duplex Fuel Oil Filter
8. Fuel Injection Pump
9. Fuel Pump Camboxes
10. Fuel Injector

J. Duoline Sheathed Fuel Injection Pipes

1. Engine Control

A.

Engine Governor and Control Equipment

Including:

PUB 3279 Part A PUB 3297 Part B PUB 3274 PUB 3298 PUB 3298

Engineers Operating Station Propulsion Control Logic Panels Series 2200 Electronic Control Unit Series 2231/1G Actuator Parts List for Actuator

A.

A.

Hydro Pnuematic Accumulator

Ivac Solenoid Valve

1. Fuel Limiter and Overspeed Trip
2. Fuel Injection Pump Control Unit
3. Air Shutdown Valve

D. Over speed Trip Unit and Drive

**J.** Lubricating System

1. Engine Lubricating Oil Circuit
2. Priming, Filtering and Sump Emptying
3. Engine Lubricating Oil Pumps
4. Hand Operated Priming Pump
5. Abany Motorised Priming Pump
6. Lubricating Oil Relief Valve
7. Lubricating Oil Filter
8. Lubricating Oil Thermostat

SECTION

**K. Cooling System**

1. Coolant Specification and Safety Data

A. Cooling Systems

1. Engine Pre-warming Unit
2. Coolant Circulating Pump
3. Sea Water Pump and Drive
4. Charge Air Heater/Cooler
5. Coolant Diversion Valve
6. Lubricating Oil Cooler

F. Heat Exchanger

1. Fuel Oil Cooler
2. Coolant Thermostat
3. **Induction and Exhaust Systems**

A Air Intake Filters

1. Air Inlet and Exhaust Manifolds

**M. Pressure Charging Equipment**

Turbocharger

N. **Engine Starting and Charging**

A. Starting Equipment

**O. Coupling**

U. **Anti-vibration mountings**

**W Wiring Diagrams**

**Y. Engine Preservation**

**Appendix A**

Approved Lubricating Oil

ILLUSTRATIONS

SECTION B

|  |  |
| --- | --- |
| FigBl | Cutaway view of engine |
|  | SECTION C |
| Fig CC.l | Drive-end gear train showing timing marks |
| Fig CC.2 | Position of fuel pump idlers when fitting camshaft |
| Fig CC 3 | Timing pump and method of camshaft adjustment |
| Fig CC.4 | Dummy injector |
|  | SECTION D |
| Fig DA.l | Barring Equipment |
|  | SECTION E |
| Fig EB.l | Compression pipe couplings |
| Fig EB.2 | Typical assembly of Type 2651 hose and fittings |
| Fig EB.3 | Assembly tools |
| Fig EB.4 | Assembly of female fittings to hose |
| Fig EB.5 | Assembly of male fittings to hose |
| Fig EB.6 | Assembly of elbow fittings to hose |
|  | SECTION F |
| Fig FA. 1 | Plan view of cylinder head |
| Fig FA. 2 | Arrangement of oil drain ferrules |
| Fig FA. 3 | Cylinder liner clamp in position |
| Fig FA.4 | Position of lever for breaking carbon seal |

|  |  |
| --- | --- |
| Fig FA.5 | Valve spring compressor in use |
| Fig FA.6 | Injector housing removal and fitting |
| Fig FA.7 | Positions of locating, coolant transfer and fuel drain ferrules and joint rings |
| Fig FA. 8 | Arrangement of cylinder head securing nuts and tightening sequence |
| Fig FA.9 | Machining dimensions for valve seat recesses and inserts |
| Fig FA. 10 | Bumping clearance tool in use |
| Fig.FA.il | Tappet adjustment indicator |
| Fig FA. 12 | Tappet Adjustment |
| Fig FB.l | Method of clamping cylinder liners |
| Fig FB.2 | Piston and Connecting Rod Removal Tools |
| Fig FB.3 | Piston and Connecting Rod Withdrawal Gear |
| Fig FB.4 | Areas for marking connecting rod. |
| Fig. FB.5 | Centre Connecting Rod Measurement |
| Fig FB 6 | Inner Track Measurement. |
| Fig FB.7 | Outer Track Measurement. |
| Fig FB.8 | Section through bearing shell. |
| Fig FB.9 | Alignment of large-end block and forked connecting rod |
| Fig FB.10 | Stretch Gauge in use |
| FigFB.il | Releasing lower setbolts, centre rod |
| Fig FB.12 | Releasing upper setbolt, centre rod |
| Fig FB.13 | Removing centre rod bearing cap |
| Fig FB.14 | Lifting gear fitted to centre rod |
| Fig FB.15 | Centre rod levered up bore,withdrawal gear fitted |
| Fig FB.16 | Releasing forked connecting rod bolts |
| Fig FB.l7 | Withdrawing forked connecting rod bolts  LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE f-i  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER /  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15. |

|  |  |
| --- | --- |
| Fig FB.18 | Lifting gear fitted to forked connecting rod |
| Fig FB.19 | Forked connecting rod levered up bore, withdrawal gear fitted |
| Fig FB.20 | Removing large-end bearing block |
| Fig FC.l | Engine camshaft, bearings and tappet housings |
| Fig FC.2 | Method of jacking tappets |
| Fig FC.3 | Withdrawing free-end camshaft bearing |
| Fig FC.4 | Marking of camshaft intermediate bearings |
| Fig FC.5 | Positioning tool for camshaft bearings |
| Fig FC.6 | Plan view of drive-end bearing housing showing bolt positions |
| FigFD.l | Arrangement of drive-end gear train |
| Fig FD.2 | Governor drive |
| Fig FD.3 | Removing and fitting coolant pump drive gearwheel |
| Fig FD4 | Centre bearing for coolant pump drive |
| Fig FD.5 | Fuel pump idler gear assembly |
| Fig FD6 | Method of removing drive-end idler gear spindles |
| Fig FD.7 | Main idler gear |
| Fig FF1 | Drive end oil sealing and flywheel mounting |
| Fig FF2 | Free-end stubshaft and oil sealing |
| Fig FF.3 | Main bearing cap removal |
| Fig FF.4 | Tool for turning out crankcase half bearing shell |
| Fig FF.5 | Checking seating of crankshaft gearwheel |
| Fig FF.6 | Pressure testing crankshaft drive-end seal |
| Fig FF.7 | Pressure testing oil thrower seal |
| Fig FF.8 | Identification of main bearing caps and tightening sequence |
| Fig FF.9 | Positioning oil thrower to crankshaft |
| 8 | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7#13 (a) 15. |

Position of crankshaft alignment indicator

Fig FF.10 Fig FF. 11 Fig. FF.12 Fig FG.l Fig. FG.2 Fig. FG.3 Fig FG.4 Fig FG.5 Fig FG.6 Fig FG.7 Fig FG.8 Fig FH.l Fig FH.2 Fig FH.3 Fig FH.4 Fig FH.5 Fig FH.6 Fig FH.7 Fig FF1.8 Fig FH.9 Fig FH.IO Fig FH.11

Crankshaft and main bearings, free-end and drive-end oil sealing

To remove and replace crankpin bore sealing cups

Torsional vibration damper

Method of mounting dampers to crankshaft

Removing drive dowels

Damper removal

Method of lifting damper

Alignment marking of crankshaft and dampers

Checking damper 'run-out'

Silicone sample container and Arrangement of damper plug

Explosion relief door

Oil drain and dipstick doors

Clamping cylinder liners

Measuring liner bore wear

Liner removal using extractor gear

Testing seal between locating ring and liner.

Cylinder liner in crankcase.

Identification of crankcase and main bearing caps.

Crankcase.

Free end cover.

Lubricating oil sump.

|  |  |
| --- | --- |
|  | SECTION G |
| Fig GB.l | Schematic arrangement of fuel oil system |
| Fig GC.l | Fuel feed pump and drive |
| Fig GC.l | Hand operated priming pump. |
| Fig GD.l | Fuel reservoir. |
| FigGE.l | Duplex fuel oil Filter. |
| Fig GF.l | Operation of fuel injection pump. |
| Fig GF.2 | Tappet removal and fitting. |
| Fig GF.3 | Pump mounted to STPC fixture for dismantling and assembly |
| Fig GF.4 | Lapping plate, to restore mating face of delivery valve seat. |
| Fig GF.5 | Meshing of control rod and sleeve. |
| Fig GF.6 | Dummy plunger fitted for barrel to pump body 'O' ring test and high pressure seal test |
| Fig GF.7 | Dummy plunger fitted for barrel to pump body face seal test. |
| Fig GF.8 | STPC fixture with setting gauge. |
| Fig GF.9 | Arrangement for checking spill cut-off point. |
| Fig GF.10 | Arrangement of High Pressure Seal Test. |
| Fig GF.ll | Arrangement of control rod adjusting screw. |
| Fig. GF.l2 | Tolerance band for new and rebuilt pumps. |
| Fig. GF.l3 | Tolerance band for service pumps. |
| Fig GF.l4 | Fuel injection pump removal and fitting. |
| Fig GF.l5 | High pressure trolley set. |
| Fig GF.l6 | Fuel Injection Pump. |
| Fig GG.l | Lifting fuel pump cambox. |
| Fig GG.2 | Method of locking camshaft. |
| Fig GG.3 | Removing and fitting drive gear. |
| 10 | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15. |

|  |  |
| --- | --- |
| Fig GG.4 | Removal of camshaft from fuel pump cambox |
| Fig GG.5 | Alignment of tappet adjustment indicator to camshaft. |
| Fig GG.6 | Alignment, fuel pump drive gear to gear hub. |
| Fig GG.7 | Fuel pump camboxes |
| Fig GH.l | Fuel Injector |
| Fig GH.2 | Fuel injector removal tool |
| Fig GH.3 | Cleaning tool - injector housing |
| Fig GH.4 | Nozzle body removal from nozzle nut |
| Fig GH.5 | Nozzle cleaning tools |
| Fig GH.6 | Nozzle flow test rig |
| Fig GH.7 | Nozzle Testmaster |
| Fig GJ.l | Assembly sheathed fuel injection piping and drain rails. |
| FigHB.l | SECTION H  Fuel limiter and overspeed shutdown unit |
| Fig HB.2 | Starting |
| Fig HB.3 | Running |
| Fig HB.4 | Overspeed trip |
| Fig HC.l | Fuel injection pump transverse linkage |
| Fig HC.2 | 'A' Bank longitudinal linkage |
| Fig HC.3 | Assembly of longitudinal linkage |
| Fig HC.4 | Setting gauge in use |
| Fig HD. 1 | Air shutdown valve |
| Fig HD.l | Overspeed Trip Unit Drive |
| Fig HD.2 | Overspeed Trip Unit |
|  | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15. |

|  |  |
| --- | --- |
|  | SECTION J |
| Fig JA.l | Diagrammatic arrangement of lubricating oil system |
| Fig JA.2 | Diagrammatic arrangement of lubricating oil system (insets) |
| Fig JC.l | Lubricating oil pump assembly |
| Fig JD.l | Hand operated priming pump |
| Fig JD.l | Motorised lubricating oil priming pump |
| Fig JD.2 | Sectional and exploded views of typical motor |
| Fig JD.3 | Detail of non-drive end bearing arrangement showing retaining clamps |
| Fig JE.l | Lubricating oil relief valve |
| Fig JF. 1 | Lubricating oil filter |
| Fig JG.l | Lubricating Oil Thermostat (Shown partly open) |
| Fig KA.l | SECTION K  Engine coolant circulation |
| Fig KA.2 | Schematic arrangement of sea water system |
| Fig KA3 | Engine coolant drain points |
| Fig KA.l | Sectional arrangement of type 'DA' hot water accelerator pumps |
| Fig KB. 1 | Coolant Circulating Pump |
| Fig KB.2 | Impeller Removal Tool |
| Fig KB.3 | Clamping Ceramic Counterface to Carrier |
| Fig KB.4 | Fitting Driving Spindle to Pump |
| Fig KC.l | Sea water pump drive |
| Fig KC.2 | Pegson sea water pump |
| FigKD.l | Combined charge air heater/cooler |
| FigKE.l | Diversion valve actuator |
| 12 | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) IS. |

|  |  |
| --- | --- |
| Fig KE.2 | Diversion valve |
| FigKF.l | Lubricating Oil Cooler |
| Fig KF.2 | Method of 'starting' tubestack |
| Fig. KF3 | Oil cooler cleaning and repair kit |
| FigKF.l | Heat exchanger |
| Fig. KF2 | Method of 'starting' tubestack |
| Fig KF.3 | Cooler cleaning and re-tubing tools |
| Fig KF.4 | Method of re-tubing |
| FigKF.l | Fuel Oil Cooler |
| Fig KG. 1 | Coolant Thermostat |
|  | SECTION L |
| Fig LA. 1 | Air intake filter |
| FigLC.l | Air inlet manifolds and piping |
| Fig LC.2 | Turbocharger inlet casings and brackets |
| Fig LC.3 | Exhaust manifolds |

SECTION M

|  |  |
| --- | --- |
| Fig M.l | Rotor blocker fitted |
| Fig M.2 | Impeller water washing |
| Fig M.3 | Withdrawal of intermediate casing |
| Fig M.4 | Withdrawal, impeller/inducer assembly |
| Fig M.5 | Bearing removal |
| Fig M.6 | Special tools |
| Fig M.7 | Section through turbocharger |

SECTION N

|  |  |
| --- | --- |
| Fig NA.l | Cutaway view of starter motor |
| Fig NA.2 | End cover removed |
| Fig NA.3 | Cover band removed |
| Fig NA.4 | Releasing brush terminals |
| Fig NA.5 | Removing field coil connection screws |
| Fig NA.6 | Removing terminal '50' |
| Fig NA.7 | Releasing connection strap |
| Fig NA.8 | Releasing brake winding connection |
| Fig NA.9 | Pinion removal |
| Fig NA.10 | Releasing engaging relay securing screws |
| Fig NA.ll | Withdrawing engaging shaft |
| Fig NA.12 | Removing D.E. bearing housing and armature |
| Fig NA.l3 | Releasing C.E. shield screws |
| Fig NA.14 | Removing ball bearing from clutch cover |
| Fig NA.l5 | Withdrawing drive spindle |
| Fig NA.l6 | Shorted turn testing |
| Fig NA.17 | Fitting self lubricating bearing |
| Fig NA.l8 | Mandrel, removing armature needle bearing |
| Fig NA.19 | Mandrel, fitting armature needle bearing |
| Fig NA.20 | Driving armature |
| Fig NA.21 | Thrust block EFAL 46 and commutator undercutting |
| Fig NA.22 | Exploded view of clutch |
| Fig NA.23 | Slackening ring nut |
| Fig NA.24 | Fitting clutch to armature |
|  | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE  PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (m) IS. |

|  |  |
| --- | --- |
| Fig NA.25 | Fitting torque meter |
| Fig NA.26 | Checking for clutch end clearance |
| Fig NA.27 | Locking ring nut |
| Fig NA.28 | Exploded view of engagement shaft |
| Fig NA.29 | Checking brake winding resistance |
| Fig NA.30 | Checking brush holder for short circuit |
| Fig NA.31 | Removing bearing locking grubscrew |
| Fig NA. 32 | Drilling for locking grubscrew |
| Fig NA.33 | Brush springs |
| Fig NA.34 | Removing roller bearing |
| Fig NA.35 | Fitting roller bearing resistance |
| Fig NA.36 | Checking winding |
| Fig NA.37 | Winding leads |
| Fig NA.38 | Section through engaging relay with dimensions |
| Fig NA.39 | Control relay assembly |
| Fig NA.40 | Armature in clamp |
| Fig NA.41 | Fitting clutch assembly |
| Fig NA.42 | Fitting bearing to clutch cover |
| Fig NA.43 | Stator frame in clamp support |
| Fig NA.44 | Fitting commutator end frame |
| Fig NA.45 | Fitting compensating washers |
| Fig NA.46 | Inserting armature into stator frame |
| Fig NA.47 | Wiring connections |
| Fig NA.48 | Fitting carbon brushes |
| Fig NA.49 | Test bench wiring diagram |
|  | LIMITED RIGHTS LEGEND  USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER  IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15. |

|  |  |
| --- | --- |
| Fig NA.50 | Lubrication points |
| Fig NA.51 | Circuit diagram of 2 off two-stage sliding gear starter motors with double starter relay and start repeat relay |
|  | SECTION 0 |
| Fig 0.1 | Coupling alignment |
| Fig 0.2 | Outer clamp studs |
| Fig 0.3 | Element Condition |
| Fig 0.4 | Section view of coupling |

SECTION U

Fig U.l Anti-vibration mounting

Fig U.2 Fitting procedure

Fig U.3 Arrangement of BOSCH electric starter motor, mounts and engine feet

TABLES

SECTION E

HOSES, TYPES, SIZES AND FITTINGS ASSEMBLY TOOLS FOR HOSES TYPES OF LOCTITE PHYSICAL PROPERTIES OF LOCTITE

TABLE EB.l TABLE EB.2 TABLE 1 TABLE 2

LIMITED RIGHTS LEGEND

USE, DUPLICATION OR DISCLOSURE OF THIS INFORMATION WHICH IS THE

PROPERTY OF GEC DIESELS LIMITED BY THE U.S. GOVERNMENT OR BOLLINGER

IS SUBJECT TO THE RESTRICTIONS SET FORTH IN DOD FAR SUPP 252.227-7013 (a) 15.